

SECTION 10 31 00

MANUFACTURED GAS FIREPLACES

Display hidden notes to specifier. (Don't know how? [Click Here](http://www.arcat.com/sd/display_hidden_notes.shtml))

*Copyright 2014 - 2016 ARCAT, Inc. - All rights reserved*

\*\* NOTE TO SPECIFIER \*\* Heat & Glo®; gas sourced fireplaces.
This section is based on the products of Heat & Glo®, which is located at:
7571 215th St. W.
Lakeville, MN 55044
Toll Free Tel: 800-669-HEAT (4328)
Email:[request info (swansonm@hearthnhome.com)](http://admin.arcat.com/users.pl?action=UserEmail&company=Heat+%26+Glo)
Web:[www.heatnglo.com](http://www.heatnglo.com)
[[Click Here](http://www.arcat.com/arcatcos/cos33/arc33011.html)] for additional information.
Heat & Glo has been the fireplace industry leader in design and innovative technology since its inception by brothers Ron and Dan Shimek in 1975. The brand pioneered direct vent gas technology in 1987 and revolutionized the way fireplaces operate in the years that followed. Today, Heat & Glo continues to develop unmatched technologies, materials and designs in a full line of fireplaces, inserts and accessories. It is the most award-winning U.S. fireplace brand and has been granted more patents than any hearth manufacturer. Heat & Glo is headquartered in Lakeville, Minn. and is a brand of Hearth and Home Technologies.

1. GENERAL
	1. SECTION INCLUDES

\*\* NOTE TO SPECIFIER \*\* Delete items below not required for project.

* + 1. Gas fireplaces and accessories including the following:
			1. Manufactured indoor gas fireplaces.
			2. Manufactured outdoor gas fireplaces.
			3. Indoor gas fireplace Inserts.
			4. Indoor gas log sets.
			5. Outdoor gas log sets.
			6. Gas fireplace mantels and fireplace surrounds.
			7. Gas fireplace accessories.
	1. RELATED SECTIONS

\*\* NOTE TO SPECIFIER \*\* Delete any sections below not relevant to this project; add others as required.

* + 1. Section 06 10 00 - Rough Carpentry.
		2. Section - .
		3. Section 22 14 13 - Facility Storm Drainage Piping.
		4. Section 26 05 00 - Common Work Results for Electrical.
	1. REFERENCES

\*\* NOTE TO SPECIFIER \*\* Delete references from the list below that are not actually required by the text of the edited section.

* + 1. ANSI Z21.44 - Gas-Fired Gravity and Fan Type Direct Vent Wall Furnaces.
		2. ANSI Z21.88 - Vented Gas Fireplace Heaters.
		3. Z21.50b - Vented Gas Fireplaces.
		4. ANSI Z223.1 - National Fuel Gas Code.
		5. CSA 2.22b - Vented Gas Fireplaces.
		6. CSA 2.33 - Vented Gas Fireplace Heaters.
		7. CAN/ULC S610 - Factory-Built Fireplaces.
		8. UL 127 - Standard for Factory-Built Fireplaces.
		9. UL 907 - Standard for Fireplace Accessories
		10. UL 1482 - Standard for Safety for Solid-Fuel Type Room Heaters.
	1. SUBMITTALS
		1. Submit under provisions of Section 01 30 00 - Administrative Requirements.
		2. Product Data: Manufacturer's data sheets on each product to be used, including:
			1. Preparation instructions and recommendations.
			2. Storage and handling requirements and recommendations.
			3. Installation methods.
		3. Shop Drawings: Provide drawing of required clearances, rough-in of enclosure and utilities.

\*\* NOTE TO SPECIFIER \*\* Delete selection samples if colors have already been selected.

* + - 1. Selection Samples: For each finish product specified, two complete sets of color chips representing manufacturer's full range of available colors and finishes.
		1. Verification Samples: For each finish product specified, two samples, minimum size 6 inches (150 mm) square representing actual product.
	1. QUALITY ASSURANCE
		1. Manufacturer Qualifications: Minimum 5 year experience manufacturing similar products.
		2. Installer Qualifications: Minimum 2 year experience installing similar products.

\*\* NOTE TO SPECIFIER \*\* Include a mock-up if the project size and/or quality warrant taking such a precaution. The following is one example of how a mock-up on a large project might be specified. When deciding on the extent of the mock-up, consider all the major different types of work on the project.

* + 1. Multiple Installation Mock-Up: Provide a mock-up for evaluation of site and framing preparation techniques and installation workmanship.
			1. Provide representative fireplace in area designated by Architect.
			2. Do not proceed with remaining units until workmanship, installation and operation are approved by Architect.
			3. Remake mock-up unit as required to produce acceptable work.
	1. PRE-INSTALLATION MEETINGS
		1. Convene minimum two weeks prior to starting work of this section.
	2. DELIVERY, STORAGE, AND HANDLING
		1. Deliver and store products in manufacturer's unopened packaging bearing the brand name and manufacturer's identification until ready for installation.
		2. Handling: Handle materials to avoid damage.
	3. PROJECT CONDITIONS
		1. Maintain environmental conditions (temperature, humidity, and ventilation) within limits recommended by manufacturer for optimum results. Do not install products under environmental conditions outside manufacturer's recommended limits.
	4. SEQUENCING
		1. Ensure that products of this section are supplied to affected trades in time to prevent interruption of construction progress.
	5. WARRANTY
		1. Warranty: Provide manufacturer's standard warranty against defects in materials and workmanship.
1. PRODUCTS
	1. MANUFACTURERS
		1. Acceptable Manufacturer: Heat & Glo®, which is located at: 7571 215th St. W.; Lakeville, MN 55044; Toll Free Tel: 800-669-HEAT (4328); Email:[request info (swansonm@hearthnhome.com)](http://admin.arcat.com/users.pl?action=UserEmail&company=Heat+%26+Glo); Web:[www.heatnglo.com](http://www.heatnglo.com)

\*\* NOTE TO SPECIFIER \*\* Delete one of the following two paragraphs; coordinate with requirements of Division 1 section on product options and substitutions.

* + 1. Substitutions: Not permitted.
		2. Requests for substitutions will be considered in accordance with provisions of Section 01 60 00 - Product Requirements.

\*\* NOTE TO SPECIFIER \*\* Delete types and models not required.

* 1. MANUFACTURED MODERN INDOOR GAS FIREPLACES
		1. Compliance - General:
			1. Comply with applicable building codes.
			2. Comply with ANSI Z21.88/CSA 2.33 or Z21.50b/CSA 2.22b.
		2. PRIMO Series - Single Sided Gas Fireplace:

\*\* NOTE TO SPECIFIER \*\* Delete control if not required.

* + - 1. Controls: RC300.

\*\* NOTE TO SPECIFIER \*\* Delete finishing package not required.

* + - 1. Finishing Package: Clean face trim kit with fade resistant black glass interior.
			2. Finishing Package: Absolute black granite surround with black granite interior.

\*\* NOTE TO SPECIFIER \*\* Delete media if not required.

* + - 1. Media: Glass Media, Crystal.
			2. Media: Glass Media, Iced Fog.
			3. Media: Glass Media, Amber.
			4. Media: Glass Media, Cobalt Blue.
			5. Media: Glass Media, Ebony.
			6. Media: Glass Media, Red.
			7. Log Set: ' The Dunes' by Elisa Carlucci modern white log set (requires glass media).

\*\* NOTE TO SPECIFIER \*\* Delete models not required.

* + - 1. Model PRIMO 48:
				1. Size: Unit Front Width: 59-1/2 inches (1511 mm). Framing Front Width: 60-1/4 inches (1530 mm). Unit Back Width: 59-1/2 inches (1511 mm). Framing Front Width: 60-1/4 inches (1530 mm). Unit Height: 30-9/16 inches (776) Framing Height: 42 inches (1067). Unit Depth: 17-3/16 inches (437 mm) Framing Depth: 18-1/4 inches (464 mm). Glass Size: 47-1/2 inches x 12-1/2 inches (1207mm X 318mm).
				2. BTU/Hour Input: 31,000 - 45,000 (NG).
			2. Model PRIMO 60:
				1. Size: Unit Front Width: 71-1/2 inches (1816 mm). Framing Front Width: 71-1/4 inches (1835 mm). Unit Back Width: 71-1/2 inches (1816 mm). Framing Front Width: 72-1/4 inches (1835mm). Unit Height: 30-9/16 inches (776) Framing Height: 48 inches (1219). Unit Depth: 17-3/16 inches (437 mm) Framing Depth: 18-1/4 inches (464 mm). Glass Size: 59-1/2 inches x 12-1/2 inches (1511mm X 318mm).
				2. BTU/Hour Input: 38,000 - 55,000 (NG).
			3. Model PRIMO 72:
				1. Size: Unit Front Width: 83-1/2 inches (2121 mm). Framing Front Width: 84-1/4 inches (2140 mm). Unit Back Width: 83-1/2 inches (2121 mm). Framing Front Width: 84-1/4 inches (2121 mm). Unit Height: 30-9/16 inches (776) Framing Height: 48 inches (1219). Unit Depth: 17-3/16 inches (437 mm) Framing Depth: 18-1/4 inches (464 mm). Glass Size: 71-1/2 inches x 12-1/2 inches (1816 mm X 318mm).
				2. BTU/Hour Input: 41,000 - 61,000 (NG).
		1. PRIMO Series - See Through Gas Fireplace:

\*\* NOTE TO SPECIFIER \*\* Delete control if not required.

* + - 1. Controls: RC300.

\*\* NOTE TO SPECIFIER \*\* Delete finishing package not required.

* + - 1. Finishing Package: Clean face trim kit with fade resistant black glass interior.
			2. Finishing Package: Absolute black granite surround with black granite interior.

\*\* NOTE TO SPECIFIER \*\* Delete media if not required.

* + - 1. Media: Glass Media, Crystal .
			2. Media: Glass Media, Iced Fog
			3. Media: Glass Media, Amber.
			4. Media: Glass Media, Cobalt Blue.
			5. Media: Glass Media, Ebony.
			6. Media: Glass Media, Red.

\*\* NOTE TO SPECIFIER \*\* Delete if not required.

* + - 1. Log Set: ' The Dunes' by Elisa Carlucci modern white log set (requires glass media).

\*\* NOTE TO SPECIFIER \*\* Delete models not required.

* + - 1. Model PRIMO 48ST:
				1. Size: Unit Front Width: 59-1/2 inches (1511 mm). Framing Front Width: 60-1/4 inches (1530 mm). Unit Back Width: 59-1/2 inches (1511 mm). Framing Front Width: 60-1/4 inches (1530 mm). Unit Height: 30-9/16 inches (776) Framing Height: 42 inches (1067). Unit Depth: 17-3/16 inches (437 mm) Framing Depth: 17 inches (432 mm). Glass Size: 47-1/2 inches x 12-1/2 inches (1207mm X 318mm).
				2. BTU/Hour Input: 31,000 - 45,000 (NG).
			2. Model PRIMO 60ST:
				1. Size: Unit Front Width: 71-1/2 inches (1816 mm). Framing Front Width: 71-1/4 inches (1835 mm). Unit Back Width: 71-1/2 inches (1816 mm). Framing Front Width: 72-1/4 inches (1835mm). Unit Height: 30-9/16 inches (776) Framing Height: 48 inches (1219). Unit Depth: 17-3/16 inches (437 mm) Framing Depth: 17 inches (432 mm). Glass Size: 59-1/2 inches x 12-1/2 inches (1511mm X 318mm).
				2. BTU/Hour Input: 38,000 - 55,000 (NG).
			3. Model PRIMO 72ST:
				1. Size: Unit Front Width: 83-1/2 inches (2121 mm). Framing Front Width: 84-1/4 inches (2140 mm). Unit Back Width: 83-1/2 inches (2121 mm). Framing Front Width: 84-1/4 inches (2121 mm). Unit Height: 30-9/16 inches (776) Framing Height: 48 inches (1219). Unit Depth: 17-3/16 inches (437 mm) Framing Depth: 17 inches (432 mm). Glass Size: 71-1/2 inches x 12-1/2 inches (1816 mm X 318mm).
				2. BTU/Hour Input: 41,000 - 61,000 (NG).

\*\* NOTE TO SPECIFIER \*\* You've never experienced modern design like this. Clean. Discreet. Luxurious. In 36, 48, 60 and 72-inch sizes. Delete if not required.

* + 1. MEZZO Single Sided (SS) Series as manufactured by Heat & Glo. Contact manufacturer.
			1. Clean, discreet, luxurious.

\*\* NOTE TO SPECIFIER \*\* Delete control if not required.

* + - 1. Controls: RC100.
			2. Controls: RC200.
			3. Controls: RC300.

\*\* NOTE TO SPECIFIER \*\* Delete fronts-doors if not required.

* + - 1. Front-Door: Brushed Nickel Clean Face Trim.
			2. Front-Door: New Bronze Clean Face Trim.
			3. Front-Door: Black Clean Face Trim.
			4. Front-Door: Loft Forge. Hand-crafted front.
			5. Front-Door: Black Quattro.
			6. Front-Door: Brushed Nickel Quattro.
			7. Front-Door: New Bronze Quattro.

\*\* NOTE TO SPECIFIER \*\* Delete media not required.

* + - 1. Media: Glass Media, Amber.
			2. Media: Glass Media, Crystal.
			3. Media: Glass Media, Cobalt Blue.
			4. Media: Glass Media, Ebony Black.
			5. Media: Glass Media, Red.
			6. Media: Iced Fog.
			7. Log Set: Natural Log Set.

\*\* NOTE TO SPECIFIER \*\* Delete models not required.

* + - 1. Model MEZZO36 SS as manufactured by Heat & Glo.
				1. Size: Unit Front Width: 46- 3/16 inches (1173 mm). Framing Front Width: 48-1/4 inches (1226 mm). Unit Back Width 46-3/16 inches (1173 mm). Framing Back Width: 48-1/4 inches (1226 mm). Unit Height: 41-3/4 inches (1060 mm). Framing Height: 42 inches (1067 mm). Unit Depth: 17-1/8 inches (435mm). Framing Depth: 18 1/4 inches (464 mm). Glass Size: 35-1/2 inches x 12-1/2 inches (902 mm x 318 mm).
				2. BTU/Hour Input: 30,000 (NG) 8.79 (Kw).
				3. Efficiency: Steady State - 49.2%, AFUE - 44.1%, Canada EnerGuide - 47.8%.
			2. Model MEZZO 48 SS as manufactured by Heat & Glo.
				1. Size: Unit Front Width: 58 inches (1473 mm). Framing Front Width: 60-1/4 inches (1530 mm). Unit Back Width 58 inches (1473 mm). Framing Back Width: 60-1/4 inches (1530 mm). Unit Height: 41-3/4 inches (1060 mm). Framing Height: 42 inches (1067 mm). Unit Depth: 17-1/8 inches (435mm). Framing Depth: 18 1/4 inches (464 mm). Glass Size: 47-1/2 inches x 12-1/2 inches (1207mm x 318 mm).
				2. BTU/Hour Input: 40,000 (NG) 11.72 (Kw).
				3. Efficiency: Steady State - 57.2%, AFUE - 46.4%, Canada EnerGuide - 53.2%.
			3. Model MEZZO 60 SS as manufactured by Heat & Glo.
				1. Size: Unit Front Width: 70 inches (1778 mm). Framing Front Width: 72-1/4 inches (1835mm). Unit Back Width 70 inches (1778 mm). Framing Back Width: 72-1/4 inches (1835 mm). Unit Height: 47-3/4 inches (1213mm). Framing Height: 48 inches (1219 mm). Unit Depth: 17-1/8 inches (435mm). Framing Depth: 18 1/4 inches (464 mm). Glass Size: 59-1/2 inches x 12-1/2 inches (1511mm x 318 mm).
				2. BTU/Hour Input: 50,000 (NG) 14.65 (Kw).
				3. Efficiency: Steady State - 63%, AFUE - 58%, Canada EnerGuide - 52.6%.
			4. Model MEZZO 72 SS as manufactured by Heat & Glo.
				1. Size: Unit Front Width: 82 inches (2083 mm). Framing Front Width: 84-1/4 inches (2140mm). Unit Back Width 82 inches (2083 mm). Framing Back Width: 84 -1/4 inches (2140 mm). Unit Height: 47-3/4 inches (1213mm). Framing Height: 48 inches (1219 mm). Unit Depth: 17-1/8 inches (435mm). Framing Depth: 18 1/4 inches (464 mm). Glass Size: 71-1/2 inches x 12-1/2 inches (1816 mm x 318 mm).
				2. BTU/Hour Input: 58,000 (NG) 16.99 (Kw).
				3. Efficiency: Steady State - 61.3%, AFUE - 56.6%, Canada Energy Guide - 51.3%.

\*\* NOTE TO SPECIFIER \*\* You've never experienced modern design like this. Clean. Discreet. Luxurious. In 36, 48, 60 and 72-inch sizes. Delete if not required.

* + 1. MEZZO See-Through (ST) Series as manufactured by Heat & Glo. Contact manufacturer.
			1. Clean, discreet, luxurious.

\*\* NOTE TO SPECIFIER \*\* Delete control if not required.

* + - 1. Controls: RC100.
			2. Controls: RC200.
			3. Controls: RC300.

\*\* NOTE TO SPECIFIER \*\* Delete fronts-doors if not required.

* + - 1. Front-Door: Brushed Nickel Clean Face Trim.
			2. Front-Door: New Bronze Clean Face Trim.
			3. Front-Door: Black Clean Face Trim.
			4. Front-Door: Loft Forge. Hand-crafted front.
			5. Front-Door: Black Quattro.
			6. Front-Door: Brushed Nickel Quattro.
			7. Front-Door: New Bronze Quattro.

\*\* NOTE TO SPECIFIER \*\* Delete media not required.

* + - 1. Media: Glass Media, Amber.
			2. Media: Glass Media, Crystal.
			3. Media: Glass Media, Cobalt Blue.
			4. Media: Glass Media, Ebony Black.
			5. Media: Glass Media, Red.
			6. Media: Iced Fog.
			7. Log Set: Natural Log Set.

\*\* NOTE TO SPECIFIER \*\* Delete models not required.

* + - 1. Model MEZZO36 ST as manufactured by Heat & Glo.
				1. Size: Unit Front Width: 46- 3/16 inches (1173 mm). Framing Front Width: 48-1/4 inches (1226 mm). Unit Back Width 46-3/16 inches (1173 mm). Framing Back Width: 48-1/4 inches (1226 mm). Unit Height: 41-3/4 inches (1060 mm). Framing Height: 42 inches (1067 mm). Unit Depth: 17-1/8 inches (435mm). Framing Depth: 17 inches (432 mm). Glass Size: 35-1/2 inches x 12-1/2 inches (902 mm x 318 mm).
				2. BTU/Hour Input: 30,000 (NG) 8.79 (Kw).
				3. Efficiency: Steady State - 49.2%, AFUE - 44.1%, Canada EnerGuide - 47.8%.
			2. Model MEZZO48 ST as manufactured by Heat & Glo.
				1. Size: Unit Front Width: 58 inches (1473 mm). Framing Front Width: 60-1/4 inches (1530 mm). Unit Back Width 58 inches (1473 mm). Framing Back Width: 60-1/4 inches (1530 mm). Unit Height: 41-3/4 inches (1060 mm). Framing Height: 42 inches (1067 mm). Unit Depth: 17-1/8 inches (435mm). Framing Depth: 17 inches (432 mm). Glass Size: 47-1/2 inches x 12-1/2 inches (1207mm x 318 mm).
				2. BTU/Hour Input: 40,000 (NG) 11.72 (Kw).
				3. Efficiency: Steady State - 57.2%, AFUE - 46.4%, Canada EnerGuide - 53.2%.
			3. Model MEZZO60 ST as manufactured by Heat & Glo.
				1. Size: Unit Front Width: 70 inches (1778 mm). Framing Front Width: 72-1/4 inches (1835mm). Unit Back Width 70 inches (1778 mm). Framing Back Width: 72-1/4 inches (1835 mm). Unit Height: 47-3/4 inches (1213mm). Framing Height: 48 inches (1219 mm). Unit Depth: 17-1/8 inches (435mm). Framing Depth: 17 inches (432 mm). Glass Size: 59-1/2 inches x 12-1/2 inches (1511mm x 318 mm).
				2. BTU/Hour Input: 50,000 (NG) 14.65 (Kw).
				3. Efficiency: Steady State - 63%, AFUE - 58%, Canada EnerGuide - 52.6%.
			4. Model MEZZO72 ST as manufactured by Heat & Glo.
				1. Size: Unit Front Width: 82 inches (2083 mm). Framing Front Width: 84-1/4 inches (2140mm). Unit Back Width 82 inches (2083 mm). Framing Back Width: 84 -1/4 inches (2140 mm). Unit Height: 47-3/4 inches (1213mm). Framing Height: 48 inches (1219 mm). Unit Depth: 17-1/8 inches (435mm). Framing Depth: 17 inches (432 mm). Glass Size: 71-1/2 inches x 12-1/2 inches (1816 mm x 318 mm).
				2. BTU/Hour Input: 58,000 (NG) 16.99 (Kw).
				3. Efficiency: Steady State - 61.3%, AFUE - 56.6%, Canada Energy Guide - 51.3%.
		1. Solaris Gas Fireplace:
			1. 32 inches (813 mm) circular viewing area.

\*\* NOTE TO SPECIFIER \*\* Trim ring styles. Delete if not required.

* + - 1. Trim Ring: Black.
			2. Trim Ring: Stone.

\*\* NOTE TO SPECIFIER \*\* Delete if not required.

* + - 1. Panels: Solaris Front Panels. Includes Top & Bottom panel set, Side panel set, and black or gloss white for the Base.

\*\* NOTE TO SPECIFIER \*\* Delete color not required.

* + - * 1. Top and Bottom Panel Sets: Ebony.
				2. Top and Bottom Panel Sets: Gloss White.

\*\* NOTE TO SPECIFIER \*\* Delete color not required.

* + - * 1. Base: Black.
				2. Base: White.
			1. Controls: WSK-21-W.

\*\* NOTE TO SPECIFIER \*\* Delete model not required.

* + - 1. Model Solaris36-ST as manufactured by Heat & Glo.
				1. Size: Unit Front Width: 47-1/2 inches (1207 mm). Framing Front Width: 47-1/2 inches (1207 mm). Unit Back Width: 47-1/2 inches (1207 mm). Framing Back Width: 47-1/2 inches (1207 mm). Unit Height: 55 inches (1397 mm). Framing Height: 55-1/4 inches (1403 mm). Unit Depth: 6-5/8 inches (168 mm). Framing Depth: 5-1/2 inches (140 mm). Glass Size: 32-1/4 inches (819 mm).
				2. BTU/Hour Input: 29,500 (8.6 kW).
			2. Model Solaris36-MR as manufactured by Heat & Glo.
				1. Size: Unit Front Width: 55 inches (1397 mm). Framing Front Width: 55-1/4 inches (1403 mm). Unit Back Width: 47-1/2 inches (1207 mm). Framing Back Width: 47-1/2 inches (1207 mm). Unit Height: 47-1/2 inches (1207 mm). Framing Height: 47-1/2 inches (1207 mm). Unit Depth: 6-5/8 inches (168 mm). Framing Depth: 5-1/2 inches (140 mm). Glass Size: 32-1/4 inches (819 mm).
				2. BTU/Hour Input: 29,500 (8.6 kW).
		1. LUX Series Gas Fireplace:

\*\* NOTE TO SPECIFIER \*\* Delete controls if not required.

* + - 1. Controls: IntelliFire Plus RC100.
			2. Controls: IntelliFire Plus RC200.
			3. Controls: IntelliFire Plus RC300.

\*\* NOTE TO SPECIFIER \*\* Delete front door style and finish not required.

* + - 1. Fronts-Doors: Black Firescreen Front.
			2. Fronts-Doors: Graphite Firescreen Front.
			3. Fronts-Doors: New Bronze Firescreen Front.
			4. Fronts-Doors: Black Modern Firescreen Front.
			5. Fronts-Doors: Fog Modern Firescreen Front.

\*\* NOTE TO SPECIFIER \*\* Delete media not required.

* + - 1. Media: Multi-Colored Ceramic Stones.
			2. Media: Glass Media, Blue.
			3. Media: Glass Media, Black.
			4. Media: Glass Media, Amber.

\*\* NOTE TO SPECIFIER \*\* Delete model not required.

* + - 1. Model Lux36 as manufactured by Heat & Glo.
				1. Size: Unit Front Width: 61 inches (1549 mm). Framing Front Width: 59-1/2 inches (1511 mm). Unit Back Width: 59-1/4 inches (1505 mm). Framing Back Width: 59-1/2 inches (1511 mm). Unit Height: 57-5/8 inches (1464 mm). Framing Height: 56 inches (1422 mm). Unit Depth: 24 inches (610 mm). Framing Depth: 24 inches (610 mm). Glass Size: 35-7/8 inches x 31-1/16 inches (911 mm x 789 mm).
				2. BTU/Hour Input: 38,000 (11.1 kW).
				3. Efficiency: Steady State 60.9%, AFUE 59.0%, Canada EnerGuide 59.4%.
			2. Model Lux42 as manufactured by Heat & Glo.
				1. Size: Unit Front Width: 67 inches (1702 mm). Framing Front Width: 65-9/16 inches (1665 mm). Unit Back Width: 65-5/16 inches (1659 mm). Framing Back Width: 56-9/16 inches (1437 mm). Unit Height: 62-5/8 inches (1591 mm). Framing Height: 61 inches (1549 mm). Unit Depth: 24 inches (610 mm). Framing Depth: 24 inches (610 mm). Glass Size: 41-7/8 inches x 36-1/16 inches (1064 mm x 916 mm).
				2. BTU/Hour Input: 49,000 (14.4 kW).
				3. Efficiency: Steady State 69.5%, AFUE 67.3%, Canada EnerGuide 66.0%.
		1. 8000 Modern Gas Fireplace:

\*\* NOTE TO SPECIFIER \*\* Delete controls if not required.

* + - 1. Controls: IntelliFire Plus RC100.
			2. Controls: IntelliFire Plus RC200.
			3. Controls: IntelliFire Plus RC300.

\*\* NOTE TO SPECIFIER \*\* Delete front door style and finish not required.

* + - 1. Fronts-Doors: Black Folio Front.
			2. Fronts-Doors: Graphite Folio Front.
			3. Fronts-Doors: New Bronze Folio Front.
			4. Fronts-Doors: Black Modern Front.
			5. Fronts-Doors: Fog Gray Modern Front.

\*\* NOTE TO SPECIFIER \*\* Delete media not required.

* + - 1. Media: Glass Media, Blue.
			2. Media: Glass Media, Black.
			3. Media: Glass Media, Amber.

\*\* NOTE TO SPECIFIER \*\* Select mantel from available in mantels Article.

* + - 1. Wood Mantels: As specified.

\*\* NOTE TO SPECIFIER \*\* Select stone surrounds from available in stone surrounds Article.

* + - 1. Stone Surrounds: As specified.

\*\* NOTE TO SPECIFIER \*\* Select cast mantels from available in cast mantels Article.

* + - 1. Cast Mantels: As specified.
			2. Model 8000CMOD-IPI as manufactured by Heat & Glo.
				1. Size: Unit Front Width: 48 inches (1219 mm). Framing Front Width: 49 inches (1245 mm). Unit Back Width: 35-1/2 inches (902 mm). Framing Back Width: 49 inches (1245 mm). Unit Height: 41-7/8 inches (1064 mm). Framing Height: 42-1/8 inches (1070 mm). Unit Depth: 21-1/2 inches (546 mm). Framing Depth: 22 inches (559 mm). Glass Size: 39 inches x 23-5/8 inches (991 mm x 600 mm).
				2. BTU/Hour Input: 32,000 (9.4 kW).
				3. Efficiency: Steady State 77.5%, AFUE 55.9%, Canada EnerGuide 61.7%.
		1. 6000 Modern Gas Fireplace:

\*\* NOTE TO SPECIFIER \*\* Delete controls if not required.

* + - 1. Controls: IntelliFire Plus RC100.
			2. Controls: IntelliFire Plus RC200.
			3. Controls: IntelliFire Plus RC300.

\*\* NOTE TO SPECIFIER \*\* Delete front door style and finish not required.

* + - 1. Fronts-Doors: Black Folio Front.
			2. Fronts-Doors: Graphite Folio Front.
			3. Fronts-Doors: New Bronze Folio Front.
			4. Fronts-Doors: Black Modern Front.
			5. Fronts-Doors: Fog Gray Modern Front.

\*\* NOTE TO SPECIFIER \*\* Delete media not required.

* + - 1. Media: Glass Media, Blue.
			2. Media: Glass Media, Black.
			3. Media: Glass Media, Amber.

\*\* NOTE TO SPECIFIER \*\* Select mantel from available in mantels Article.

* + - 1. Wood Mantels: As specified.

\*\* NOTE TO SPECIFIER \*\* Select stone surrounds from available in stone surrounds Article.

* + - 1. Stone Surrounds: As specified.

\*\* NOTE TO SPECIFIER \*\* Select cast mantels from available in cast mantels Article.

* + - 1. Cast Mantels: As specified.
			2. Model 6000CMOD-IPI as manufactured by Heat & Glo.
				1. Size: Unit Front Width: 41 inches (1041 mm). Framing Front Width: 42 inches (1067 mm). Unit Back Width: 28-1/2 inches (724 mm). Framing Back Width: 42 inches (1067 mm). Unit Height: 39-7/8 inches (1013 mm). Framing Height: 40-1/8 inches (1019 mm). Unit Depth: 21-1/2 inches (546 mm). Framing Depth: 22 inches (559 mm). Glass Size: 32 inches x 21-1/2 inches (813 mm x 546 mm).
				2. BTU/Hour Input: 28,000 (8.2 kW).
				3. Efficiency: Steady State 78.5%, AFUE 61.1%, Canada EnerGuide 63%.
		1. Everest Gas Fireplace:

\*\* NOTE TO SPECIFIER \*\* Delete controls if not required.

* + - 1. Control: WSK21.
			2. Control: Smart-Stat.

\*\* NOTE TO SPECIFIER \*\* Delete cast surround if not required.

* + - 1. Cast Surround: Atlas Cast Surround - Atlas Gray.
			2. Cast Surround: Atlas Cast Surround - Atlas Greige.
			3. Model Everest as manufactured by Heat & Glo.
				1. Size: Unit Front Width: 34-1/8 inches (867 mm). Framing Front Width: 35-1/8 inches (892 mm). Unit Back Width: 17-7/8 inches (454 mm). Framing Back Width: 35-1/16 inches (891 mm). Unit Height: 49-7/8 inches (1267 mm). Framing Height: 50-1/2 inches (1283 mm). Unit Depth: 20-7/8 inches (530 mm). Framing Depth: 21-3/8 inches (543 mm). Glass Size: 26-7/8 inches x 33-3/8 inches (683 mm x 848 mm).
				2. BTU/Hour Input: 33,000 (9.7 kW) (NG).
				3. Efficiency: Steady State 71.5%, AFUE 43.6%, Canada EnerGuide 46.3%.
		1. REVO Gas Fireplace:

\*\* NOTE TO SPECIFIER \*\* Delete control if not required.

* + - 1. Controls: IntelliFire Plus RC100.
			2. Controls: IntelliFire Plus RC200.
			3. Controls: IntelliFire Plus RC300.

\*\* NOTE TO SPECIFIER \*\* Delete fronts-doors not required.

* + - 1. Front - Door: Black Frame Front.
			2. Front - Door: Graphite Frame Front.
			3. Front - Door: New Bronze Frame Front.
			4. Front - Door: Black Radius Front.
			5. Front - Door: Graphite Radius Front.
			6. Front - Door: New Bronze Radius Front.
			7. Front - Door: Black Studio Front with Panels.
			8. Front - Door: Fog Gray Studio Front with Panels.

\*\* NOTE TO SPECIFIER \*\* Delete panels not required.

* + - 1. Panels: Glass, Gloss Black.
			2. Panels: Stainless Steel.
			3. Panels: Gloss White.

\*\* NOTE TO SPECIFIER \*\* Delete decorative knobs not required.

* + - 1. Decorative Knobs: Gloss Black.
			2. Decorative Knobs: Gray.
			3. Decorative Knobs: White.

\*\* NOTE TO SPECIFIER \*\* Insert color. Delete if not required.

* + - 1. Ambient Light:

\*\* NOTE TO SPECIFIER \*\* Delete model not required.

* + - 1. Model Revo H31 as manufactured by Heat & Glo.
				1. Size: Unit Front Width: 38-5/16 inches (973 mm). In-Wall Framing Front Width: 39-1/8 inches (994 mm). Unit Back Width: 38-5/16 inches (973 mm). In-Wall Framing Back Width: 39-1/8 inches (994 mm). Unit Height: 29-3/16 inches (741 mm). In-Wall Framing Height: 37-1/2 inches (953 mm). Unit Depth: 6-9/16 inches (243 mm). In-Wall Framing Depth: 2-5/8 inches (67 mm). Glass Size: 31 inches x 17 inches (787 mm x 432 mm).
				2. BTU/Hour Input: 24,000 (7 kW).
				3. Efficiency: Steady State 68.4%, AFUE 66.3%, Canada EnerGuide 67.5%.
			2. Model Revo S21 as manufactured by Heat & Glo.
				1. Size: Unit Front Width: 28-7/16 inches (722 mm). In-Wall Framing Front Width: 31-1/2 inches (800 mm). Unit Back Width: 28-7/16 inches (722 mm). In-Wall Framing Back Width: 31-1/2 inches (800 mm). Unit Height: 33-5/8 inches (854 mm). In-Wall Framing Height: 40-1/2 inches (1029 mm). Unit Depth: 6-9/16 inches (167 mm). In-Wall Framing Depth: 2-5/8 inches (67 mm). Glass Size: 21-3/16 inches x 21-3/8 inches (538 mm x 543 mm).
				2. BTU/Hour Input: 18,800 (5.5 kW).
				3. Efficiency: Steady State 63%, AFUE 62.7%, Canada EnerGuide 64.5%.
			3. Model Revo V12 as manufactured by Heat & Glo.
				1. Size: Unit Front Width: 19-5/16 inches (508 mm). In-Wall Framing Front Width: 20-1/8. Unit Back Width: 19-5/16 inches (491 mm). In-Wall Framing Back Width: 20-1/8 inches (511 mm). Unit Height: 36-1/8 inches (918 mm). In-Wall Framing Height: 44-5/8 inches (1133 mm). Unit Depth: 6-9/16 inches (167 mm). In-Wall Framing Depth: 2-5/8 inches (67 mm). Glass Size: 12 inches x 24 inches (305 mm x 610 mm).
				2. BTU/Hour Input: 14,250 (4.2 kW).
				3. Efficiency: Steady State 63.7%, AFUE 61.8%, Canada EnerGuide 60.2%.
		1. ST-550TM See-Through Gas Fireplace:

\*\* NOTE TO SPECIFIER \*\* Delete controls if not required.

* + - 1. Controls: Smart-Stat.

\*\* NOTE TO SPECIFIER \*\* Delete front door style and finish not required.

* + - 1. Fronts-Doors: Black Modern Front.
			2. Fronts-Doors: Graphite Modern Front.
			3. Fronts-Doors: New Bronze Modern Front.
			4. Fronts-Doors: Gray Modern Front.

\*\* NOTE TO SPECIFIER \*\* Delete media not required.

* + - 1. Media: Glass Media, Crystal.
			2. Media: Glass Media, Blue.
			3. Media: Glass Media, Black.
			4. Media: Glass Media, Amber.
			5. Model ST-550TM as manufactured by Heat & Glo.
				1. Size: Unit Front Width: 37-5/8 inches (956 mm).Framing Front Width: 38-1/8 inches (968 mm). Unit Back Width: 37-5/8 inches (956 mm). Framing Back Width: 38-1/8 inches (968 mm). Unit Height: 41-1/4 inches (1048 mm). Framing Height: 41-1/2 inches (1054 mm). Unit Depth: 16 inches (406 mm). Framing Depth: 15 inches (381 mm).Glass Size: 31 inches x 21 inches (787 mm x 533 mm).
				2. BTU/Hour Input: 22,000 (6.4 kW).
		1. Cosmo Series Gas Fireplace:

\*\* NOTE TO SPECIFIER \*\* Delete controls if not required.

* + - 1. Controls: Smart-Stat.
			2. Controls: Included WSK21.

\*\* NOTE TO SPECIFIER \*\* Delete front door style and finish not required.

* + - 1. Fronts-Doors: Graphite Martini Front.
			2. Fronts-Doors: New Bronze Martini Front.
			3. Fronts-Doors: Fog Gray Martini Front.
			4. Fronts-Doors: Graphite Tonic Front.
			5. Fronts-Doors: New Bronze Tonic Front.
			6. Fronts-Doors: Fog Gray Tonic Front.

\*\* NOTE TO SPECIFIER \*\* Delete media not required.

* + - 1. Media: Glass Media, Crystal.
			2. Media: Glass Media, Blue.
			3. Media: Glass Media, Black.
			4. Media: Glass Media, Amber.
			5. Media: Glass Beads, White.
			6. Media: Glass Beads, Black.
			7. Media: Glass Beads, Clear.
			8. Media: Multi-colored stones.

\*\* NOTE TO SPECIFIER \*\* Log set. Refer to manufacturer's literature for applicable sets for the model. Delete if not required.

* + - 1. Log Set:

\*\* NOTE TO SPECIFIER \*\* Delete if not required.

* + - 1. Liner: Reflective Black ceramic liner.
			2. Model Cosmo 32 as manufactured by Heat & Glo.
				1. Size: Unit Front Width: 36-3/4 inches (933 mm). Framing Front Width: 37-3/4 inches (959 mm). Unit Back Width: 25-3/4 inches (654 mm). Framing Back Width: 37-3/4 inches (959 mm). Unit Height: 36 inches (914 mm). Framing Height: 36-1/2 inches (927 mm). Unit Depth: 18-5/16 inches (465 mm). Framing Depth: 18-1/4 inches (464 mm). Glass Size: 27-1/4 inches x 13-1/4 inches (692 mm x 337 mm).
				2. BTU/Hour Input: 20,000 (5.9 kW).
				3. Efficiency: Steady State 60%, AFUE 57%, Canada EnerGuide 57%.
			3. Model Cosmo 42 as manufactured by Heat & Glo.
				1. Size: Unit Front Width: 48 inches (1219 mm). Framing Front Width: 50 inches (1270 mm). Unit Back Width: 37-3/4 inches (959 mm). Framing Back Width: 50 inches (1270 mm). Unit Height: 41-3/4 inches (1060 mm). Framing Height: 42-1/4 inches (1073 mm). Unit Depth: 16-3/4 inches (425 mm). Framing Depth: 18-1/4 inches (464 mm). Glass Size: 39-1/16 inches x 13-1/4 inches (992 mm x 337 mm).
				2. BTU/Hour Input: 26,000 (7.6 kW).
				3. Efficiency: Steady State 73%, AFUE 56%, Canada EnerGuide 57%.
	1. MANUFACTURED TRADITIONAL INDOOR GAS FIREPLACES
		1. Compliance - General:
			1. Comply with applicable building codes.
			2. Comply with ANSI Z21.88/CSA 2.33 or Z21.50b/CSA 2.22b.
		2. TRUE Series Gas Fireplace:

\*\* NOTE TO SPECIFIER \*\* Delete if controls not required.

* + - 1. Controls: IntelliFire Plus RC100.
			2. Controls: IntelliFire Plus RC200.
			3. Controls: IntelliFire Plus RC300.

\*\* NOTE TO SPECIFIER \*\* Delete front door style and finish not required.

* + - 1. Fronts-Doors: Forge Front.
			2. Fronts-Doors: Black Firescreen Front.
			3. Fronts-Doors: Graphite Firescreen Front.
			4. Fronts-Doors: New Bronze Firescreen Front.
			5. Fronts-Doors: Black Arched Firescreen Front.
			6. Fronts-Doors: Graphite Arched Firescreen Front.
			7. Fronts-Doors: New Bronze Arched Firescreen Front.

\*\* NOTE TO SPECIFIER \*\* Delete refractory not required.

* + - 1. Refractory: Stratford.
			2. Refractory: Herringbone.
			3. Refractory: Castlewood.

\*\* NOTE TO SPECIFIER \*\* Select cast mantels from available in cast mantels Article.

* + - 1. Cast Mantels: As specified.

\*\* NOTE TO SPECIFIER \*\* Select mantel shelves from available in mantel shelve Article.

* + - 1. Mantel Shelf: As specified.

\*\* NOTE TO SPECIFIER \*\* Delete model not required.

* + - 1. Model TRUE-36 as manufactured by Heat & Glo.
				1. Size: Unit Front Width: 61 inches (1549 mm). Framing Front Width: 59-1/2 inches (1511 mm). Unit Back Width: 59-1/4 inches (1505 mm). Framing Back Width: 59-1/2 inches (1511 mm). Unit Height: 57-5/8 inches (1464 mm). Framing Height: 56 inches (1422 mm). Unit Depth: 24 inches (610 mm). Framing Depth: 24 inches (610 mm). Glass Size: 35-7/8 inches x 31-1/16 inches (911 mm x 789 mm).
				2. BTU/Hour Input: 28,000 - 45,000 (8.2 - 13.2 kW).
				3. Efficiency: Steady State 76.2%, AFUE 51.9%, Canada EnerGuide 57.6%.
			2. Model TRUE-42 as manufactured by Heat & Glo.
				1. Size: Unit Front Width: 67 inches (1702 mm). Framing Front Width: 65-9/16 inches (1665 mm). Unit Back Width: 65-5/16 inches (1659 mm). Framing Back Width: 69-9/16 inches (1767 mm). Unit Height: 62-5/8 inches (1591 mm). Framing Height: 61 inches (1549 mm). Unit Depth: 24 inches (610 mm). Framing Depth: 24 inches (610 mm). Glass Size: 41-7/8 inches x 36-1/16 inches (1064 mm x 916 mm).
				2. BTU/Hour Input: 30,000 - 55,000 (8.8 - 16.1 kW).
				3. Efficiency: Steady State 77.2%, AFUE 67.0%, Canada EnerGuide 67.0%.
			3. Model TRUE-50 as manufactured by Heat & Glo.
				1. Size: Unit Front Width: 75 inches (1905 mm). Framing Front Width: 73-5/8 inches (1870 mm). Unit Back Width: 73-5/16 inches (1862 mm). Framing Back Width: 73-5/8 inches (1870 mm). Unit Height: 66-5/8 inches (1692 mm). Framing Height: 65 inches (1651 mm). Unit Depth: 24 inches (610 mm). Framing Depth: 24 inches (610 mm). Glass Size: 49-7/8 inches x 40-1/16 inches (1267 mm x 1018 mm).
				2. BTU/Hour Input: 37,000 - 65,000 (10.8 - 19 kW).
				3. Efficiency: Steady State 68.9%, AFUE 66.8%, Canada EnerGuide 69.1%.
		1. Escape See-Through Gas Fireplace:

\*\* NOTE TO SPECIFIER \*\* Delete if not required.

* + - 1. Control: IntelliFire Plus RC300.

\*\* NOTE TO SPECIFIER \*\* Delete fronts and doors not required.

* + - 1. Fronts-Doors: Black Non-Operable Firescreen Front.
			2. Fronts-Doors: Bronze Non-Operable Firescreen Front.
			3. Fronts-Doors: Black Arched Firescreen Front.
			4. Fronts-Doors: Graphite Arched Firescreen Front.
			5. Fronts-Doors: New Bronze Arched Firescreen Front.

\*\* NOTE TO SPECIFIER \*\* Accent your firescreen front with decorative companions.

* + - 1. Firescreen Companion: Black Prairie Ridge Companions.
			2. Firescreen Companion: Bronze Prairie Ridge Companions.
			3. Firescreen Companion: Andirons.

\*\* NOTE TO SPECIFIER \*\* Delete refractory not required.

* + - 1. Refractory: Stratford Traditional.

\*\* NOTE TO SPECIFIER \*\* Select cast mantels from available in cast mantels Article.

* + - 1. Cast Mantels: As specified.

\*\* NOTE TO SPECIFIER \*\* Select mantel shelves from available in mantel shelve Article.

* + - 1. Mantel Shelf: As specified.
			2. Model Escape-ST as manufactured by Heat & Glo.
				1. Size: Unit Front Width: 59-15/16 (1522 mm). Framing Front Width: 60-1/4 inches (1530 mm). Unit Back Width: 59-15/16 inches (1522 mm). Framing Back Width: 60-1/4 inches (1530 mm). Unit Height: 46-3/8 inches (1178 mm). Framing Height: 46-1/2 inches (1181 mm). Unit Depth: 30 inches (762 mm). Framing Depth: 30 inches (762 mm). Glass Size: 39-7/16 inches x 35-1/8 inches (1002 mm x 892 mm).
				2. BTU/Hour Input: 57,500 (16.9 kW).
				3. Efficiency: Steady State 75%, AFUE 62%, Canada EnerGuide 60%.
		1. Cerona Series Gas Fireplace:

\*\* NOTE TO SPECIFIER \*\* Delete if controls not required.

* + - 1. Controls: Includes WSK-MLT Wall Switch.
			2. Controls: RCT-MLT.

\*\* NOTE TO SPECIFIER \*\* Delete fronts-doors if not required.

* + - 1. Front-Door: Black Valencia Arched Front.
			2. Front-Door: Graphite Valencia Arched Front.
			3. Front-Door: New Bronze Valencia Arched Front.
			4. Front-Door: Black Chateau Arched Front.
			5. Front-Door: Graphite Chateau Arched Front.
			6. Front-Door: New Bronze Chateau Arched Front.
			7. Front-Door: Black Chateau Deluxe Arched Front.
			8. Front-Door: Graphite Chateau Deluxe Arched Front.
			9. Front-Door: New Bronze Chateau Deluxe Arched Front.

\*\* NOTE TO SPECIFIER \*\* Delete if not required.

* + - 1. Trim: Cast arch trim stone.

\*\* NOTE TO SPECIFIER \*\* Select mantel from available in mantel Article.

* + - 1. Mantel: As specified.

\*\* NOTE TO SPECIFIER \*\* Delete model not required.

* + - 1. Model CERONA-36 as manufactured by Heat & Glo.
				1. Size: Unit Front Width: 41-1/8 inches (1045 mm). Framing Front Width: 42-1/8 inches (1070 mm). Unit Back Width: 28-1/2 inches (724 mm). Framing Back Width: 42-1/8 inches (1070 mm). Unit Height: 49-7/8 inches (1267 mm). Framing Height: 50-1/2 inches (1283 mm). Unit Depth: 21-3/4 inches (552 mm). Framing Depth: 22-1/4 inches (565 mm). Glass Size: 30-1/4 inches x 23-1/2 inches (768 mm x 597 mm).
				2. BTU/Hour Input: 37,500 (11 kW).
			2. Model CERONA-42 as manufactured by Heat & Glo.
				1. Size: Unit Front Width: 48-1/8 inches (1222 mm). Framing Front Width: 49-1/8 inches (1248 mm). Unit Back Width: 35-3/8 inches (899 mm). Framing Back Width: 49-1/8 inches (1248 mm). Unit Height: 54 inches (1372 mm). Framing Height: 54-1/2 inches (1384 mm). Unit Depth: 21-3/4 inches (552 mm). Framing Depth: 22-1/4 inches (565 mm). Glass Size: 35-7/8 inches x 27-3/4 inches (911 mm x 705 mm).
				2. BTU/Hour Input: 48,000 (14.1 kW).
		1. Energy Pro Gas Fireplace:

\*\* NOTE TO SPECIFIER \*\* Delete if not required.

* + - 1. Control: Wireless Thermostat.

\*\* NOTE TO SPECIFIER \*\* Delete fronts and doors not required.

* + - 1. Fronts-Doors: Black Folio Front.
			2. Fronts-Doors: Graphite Folio Front.
			3. Fronts-Doors: New Bronze Folio Front.
			4. Fronts-Doors: Forge Front. Forge front made from hand-crafted hammered steel.

\*\* NOTE TO SPECIFIER \*\* Delete refractory not required.

* + - 1. Refractory: Brick Refractory.

\*\* NOTE TO SPECIFIER \*\* Select mantel from available in mantels Article. Bella cabinet not available for the Caliber nXt Series.

* + - 1. Wood Mantels: As specified.

\*\* NOTE TO SPECIFIER \*\* Select stone surrounds from available in stone surrounds Article.

* + - 1. Stone Surrounds: As specified.

\*\* NOTE TO SPECIFIER \*\* Select cast mantels from available in cast mantels Article.

* + - 1. Cast Mantels: As specified.

\*\* NOTE TO SPECIFIER \*\* Select mantel shelves from available in mantel shelve Article.

* + - 1. Mantel Shelf: As specified.
			2. Model Energy Pro as manufactured by Heat & Glo.
				1. Size: Unit Front Width: 40-15/16 inches (1040 mm). Framing Front Width: 42 inches (1067 mm). Unit Back Width: 41 inches (1041 mm). Framing Back Width: 42 inches (1067 mm).Unit Height: 43-11/16 inches (1110 mm). Framing Height: 44 inches (1118 mm). Unit Depth: 27-1/2 inches (699 mm). Framing Depth: 28 inches (711 mm). Glass Size: 31 inches x 35-1/4 inches (787 mm x 895 mm).
				2. BTU/Hour Input: 36,000 (10.6 kW).
				3. Efficiency: Steady State 89.8%, AFUE 92.6%, Canada EnerGuide 86.3%.
		1. 8000 Series Gas Fireplace:

\*\* NOTE TO SPECIFIER \*\* Delete controls if not required.

* + - 1. Controls: IntelliFire Plus RC100.
			2. Controls: IntelliFire Plus RC200.
			3. Controls: IntelliFire Plus RC300.

\*\* NOTE TO SPECIFIER \*\* Delete fronts-doors if not required.

* + - 1. Front-Door: Black Clean Face Front.
			2. Front-Door: Graphite Clean Face Front.
			3. Front-Door: New Bronze Clean Face Front.
			4. Front-Door: Black Galleria Arched Front.
			5. Front-Door: Graphite Galleria Arched Front.
			6. Front-Door: New Bronze Galleria Arched Front.
			7. Front-Door: Black Halston Front.
			8. Front-Door: Graphite Halston Front.
			9. Front-Door: New Bronze Halston Front.
			10. Front-Door: Chateau Forge Front, hand-crafted with forged bars and straps, overlap front in natural finish.
			11. Front-Door: Black Chateau Front.
			12. Front-Door: Graphite Chateau Front.
			13. Front-Door: New Bronze Chateau Front.
			14. Front-Door: Black Arcadia Front.
			15. Front-Door: Graphite Arcadia Front.
			16. Front-Door: New Bronze Arcadia Front.
			17. Front-Door: Black Folio Front.
			18. Front-Door: Graphite Folio Front.
			19. Front-Door: New Bronze Folio Front.
			20. Refractory: Stratford Brick.

\*\* NOTE TO SPECIFIER \*\* Select mantel from available in mantels Article.

* + - 1. Wood Mantels: As specified.

\*\* NOTE TO SPECIFIER \*\* Select stone surrounds from available in stone surrounds Article.

* + - 1. Stone Surrounds: As specified.

\*\* NOTE TO SPECIFIER \*\* Select cast mantels from available in cast mantels Article.

* + - 1. Cast Mantels: As specified.

\*\* NOTE TO SPECIFIER \*\* Select mantel shelf from available in mantel shelf Article.

* + - 1. Mantel Shelf: As specified.

\*\* NOTE TO SPECIFIER \*\* Delete model not required.

* + - 1. Model 8000C as manufactured by Heat & Glo.
				1. Size: Unit Front Width: 48 inches (1219 mm).Framing Front Width: 49 inches (1245 mm). Unit Back Width: 35-1/2 inches (902 mm). Framing Back Width: 49 inches (1245 mm). Unit Height: 41-7/8 inches (1064 mm). Framing Height: 42-1/8 inches (1070 mm). Unit Depth: 21 inches (533 mm). Framing Depth: 22 inches (559 mm). Glass Size: 39 inches x 23-5/8 inches (991 mm x 600 mm).
				2. BTU/Hour Input: 35,000 (10.3 kW).
				3. Efficiency: Steady State 83%, AFUE 63%, Canada EnerGuide 67%.
			2. Model 8000CL as manufactured by Heat & Glo.
				1. Size: Unit Front Width: 48 inches (1219 mm). Framing Front Width: 49 inches (1245 mm). Unit Back Width: 35-1/2 inches (902 mm). Framing Back Width: 49 inches (1245 mm). Unit Height: 41-7/8 inches (1064 mm). Framing Height: 42-1/8 inches (1070 mm). Unit Depth: 21 inches (533 mm). Framing Depth: 22 inches (559 mm). Glass Size: 39 inches x 23-5/8 inches (991 mm x 600 mm).
				2. BTU/Hour Input: 40,000 (11.7 kW).
				3. Efficiency: Steady State 83%, AFUE 65%, Canada EnerGuide 65%.
			3. Model 8000CLX as manufactured by Heat & Glo.
				1. Size: Unit Front Width: 48 inches (1219 mm). Framing Front Width: 49 inches (1245 mm). Unit Back Width: 35-1/2 inches (902 mm). Framing Back Width: 49 inches (1245 mm). Unit Height: 41-7/8 inches (1064 mm). Framing Height: 42-1/8 inches (1070 mm). Unit Depth: 21 inches (533 mm). Framing Depth: 22 inches (559 mm). Glass Size: 39 inches x 23-5/8 inches (991 mm x 600 mm).
				2. BTU/Hour Input: 45,000 (13.2 kW).
				3. Efficiency: Steady State 84%, AFUE 66%, Canada EnerGuide 68%.
		1. 6000 Series Gas Fireplace:

\*\* NOTE TO SPECIFIER \*\* Delete controls if not required.

* + - 1. Controls: IntelliFire Plus RC100.
			2. Controls: IntelliFire Plus RC200.
			3. Controls: IntelliFire Plus RC300.

\*\* NOTE TO SPECIFIER \*\* Delete fronts-doors if not required.

* + - 1. Front-Door: Black Clean Face Front.
			2. Front-Door: Graphite Clean Face Front.
			3. Front-Door: New Bronze Clean Face Front.
			4. Front-Door: Black Galleria Arched Front.
			5. Front-Door: Graphite Galleria Arched Front.
			6. Front-Door: New Bronze Galleria Arched Front.
			7. Front-Door: Black Halston Front.
			8. Front-Door: Graphite Halston Front.
			9. Front-Door: New Bronze Halston Front.
			10. Front-Door: Chateau Forge Front, hand-crafted with forged bars and straps, overlap front in natural finish.
			11. Front-Door: Black Chateau Front.
			12. Front-Door: Graphite Chateau Front.
			13. Front-Door: New Bronze Chateau Front.
			14. Front-Door: Black Arcadia Front.
			15. Front-Door: Graphite Arcadia Front.
			16. Front-Door: New Bronze Arcadia Front.
			17. Front-Door: Black Folio Front.
			18. Front-Door: Graphite Folio Front.
			19. Front-Door: New Bronze Folio Front.
			20. Refractory: Stratford Brick.

\*\* NOTE TO SPECIFIER \*\* Select mantel from available in mantels Article.

* + - 1. Wood Mantels: As specified.

\*\* NOTE TO SPECIFIER \*\* Select stone surrounds from available in stone surrounds Article.

* + - 1. Stone Surrounds: As specified.

\*\* NOTE TO SPECIFIER \*\* Select cast mantels from available in cast mantels Article.

* + - 1. Cast Mantels: As specified.

\*\* NOTE TO SPECIFIER \*\* Select mantel shelf from available in mantel shelf Article.

* + - 1. Mantel Shelf: As specified.

\*\* NOTE TO SPECIFIER \*\* Delete model not required.

* + - 1. Model 6000C as manufactured by Heat & Glo.
				1. Size: Unit Front Width: 41 inches (1041 mm). Framing Front Width: 42 inches (1067 mm). Unit Back Width: 28-1/2 inches (724 mm). Framing Back Width: 42 inches (1067 mm). Unit Height: 39-7/8 inches (1013 mm). Framing Height: 40-1/8 inches (1019 mm). Unit Depth: 21 inches (533 mm). Framing Depth: 22 inches (559 mm). Glass Size: 32 inches x 21-1/2 inches (813 mm x 546 mm).
				2. BTU/Hour Input: 30,000 (8.8 kW).
				3. Efficiency: Steady State 81%, AFUE 60%, Canada EnerGuide 64%.
			2. Model 6000CL as manufactured by Heat & Glo.
				1. Size: Unit Front Width: 41 inches (1041 mm). Framing Front Width: 42 inches (1067 mm). Unit Back Width: 28-1/2 inches (724 mm). Framing Back Width: 42 inches (1067 mm). Unit Height: 39-7/8 inches (1013 mm). Framing Height: 40-1/8 inches (1019 mm). Unit Depth: 21 inches (533 mm). Framing Depth: 22 inches (559 mm). Glass Size: 32 inches x 21-1/2 inches (813 mm x 546 mm).
				2. BTU/Hour Input: 35,000 (10.3 kW).
				3. Efficiency: Steady State 82%, AFUE 64%, Canada EnerGuide 68%.
			3. Model 6000CLX as manufactured by Heat & Glo.
				1. Size: Unit Front Width: 41 inches (1041 mm). Framing Front Width: 42 inches (1067 mm). Unit Back Width: 28-1/2 inches (724 mm). Framing Back Width: 42 inches (1067 mm). Unit Height: 39-7/8 inches (1013 mm). Framing Height: 40-1/8 inches (1019 mm). Unit Depth: 21 inches (533 mm). Framing Depth: 22 inches (559 mm). Glass Size: 32 inches x 21-1/2 inches (813 mm x 546 mm).
				2. BTU/Hour Input: 40,000 (11.7 kW).
				3. Efficiency: Steady State 83%, AFUE 65%, Canada EnerGuide 67%.
		1. Pier-36TR Multi-Sided Gas Fireplace:

\*\* NOTE TO SPECIFIER \*\* Delete controls if not required.

* + - 1. Controls: WSK200.
			2. Controls: Smart-Stat.
			3. Controls: WSK-MLT Wall Switch.
			4. Controls: RCT-MLT.

\*\* NOTE TO SPECIFIER \*\* Delete fronts-doors if not required.

* + - 1. Front-Door: Black Arcadia Front.
			2. Front-Door: Graphite Arcadia Front.
			3. Front-Door: New Bronze Arcadia Front.
			4. Front-Door: Black Folio Front.
			5. Front-Door: Graphite Folio Front.
			6. Front-Door: New Bronze Folio Front.
			7. Front-Door: Black Chateau Front.
			8. Front-Door: Graphite Chateau Front.
			9. Front-Door: New Bronze Chateau Front.

\*\* NOTE TO SPECIFIER \*\* Select mantels from available in mantels Article.

* + - 1. Mantels: As specified.
			2. Model Pier-36TR as manufactured by Heat & Glo.
				1. Size: Unit Front Width: 40-1/2 inches (1029 mm). Framing Front Width: 40 inches (1016 mm). Unit Back Width: 40-1/2 inches (1029 mm). Framing Back Width: 40 inches (1016 mm). Unit Height: 38 inches (965 mm). Framing Height: 38-1/8 inches (968 mm). Unit Depth: 24 inches (610 mm). Framing Depth: 23 inches (584 mm). Glass Size: 36 inches x 24-1/2 inches (914 mm x 622 mm).
				2. BTU/Hour Input: 37,000 (10.9 kW).
		1. Corner Series Gas Fireplace:

\*\* NOTE TO SPECIFIER \*\* Delete controls if not required.

* + - 1. Controls: WSK200.
			2. Controls: RCT-MLT.
			3. Controls: WSK-MLT Wall Switch.

\*\* NOTE TO SPECIFIER \*\* Delete front door style and finish not required.

* + - 1. Fronts-Doors: Black Folio Front.
			2. Fronts-Doors: Graphite Folio Front.
			3. Fronts-Doors: New Bronze Folio Front.
			4. Model LCOR-36TRB as manufactured by Heat & Glo.
			5. Model RCOR-36TRB as manufactured by Heat & Glo.
				1. Size: Unit Front Width: 40-1/2 inches (1029 mm). Framing Front Width: 40 inches (1016 mm). Unit Back Width: 40-1/2 inches (1029 mm). Framing Back Width: 40 inches (1016 mm). Unit Height: 38 inches (965 mm). Framing Height: 38-1/8 inches (968 mm). Unit Depth: 24-1/2 inches (622 mm). Framing Depth: 24 inches (610 mm). Glass Size: 36 inches x 24-1/2 inches (914 mm x 622 mm).
				2. BTU/Hour Input: 26,000-37,000 (7.6 - 10.8 kW).
				3. Efficiency: Steady State 72%, AFUE 59%, Canada EnerGuide 61%.
		1. ST-36 See-Through Gas Fireplace:

\*\* NOTE TO SPECIFIER \*\* Delete controls if not required.

* + - 1. Controls: WSK200.
			2. Controls: Smart-Stat.
			3. Controls: WSK-MLT Wall Switch.
			4. Controls: RCT-MLT.
			5. Controls: WSK21.

\*\* NOTE TO SPECIFIER \*\* Delete fronts and doors not required.

* + - 1. Front-Door: Black Galleria Front.
			2. Front-Door: Graphite Galleria Front.
			3. Front-Door: New Bronze Galleria Front.
			4. Front-Door: Black Chateau Front.
			5. Front-Door: Graphite Chateau Front.
			6. Front-Door: New Bronze Chateau Front.
			7. Front-Door: Black Arcadia Front.
			8. Front-Door: Graphite Arcadia Front.
			9. Front-Door: New Bronze Arcadia Front.
			10. Front-Door: Black Folio Front.
			11. Front-Door: Graphite Folio Front.
			12. Front-Door: New Bronze Folio Front.

\*\* NOTE TO SPECIFIER \*\* Select mantels from available in mantels Article.

* + - 1. Mantels: As specified.

\*\* NOTE TO SPECIFIER \*\* Select mantel shelves from available in mantel shelve Article.

* + - 1. Mantel Shelf: As specified.
			2. Model ST-36TR as manufactured by Heat & Glo.
				1. Size: Unit Front Width: 42-1/2 inches (1080 mm). Framing Front Width: 43 inches (1092 mm). Unit Back Width: 42-1/2 inches (1080 mm). Framing Back Width: 43 inches (1092 mm). Unit Height: 38 inches (965 mm). Framing Height: 38-1/2 inches (978 mm). Unit Depth: 24 inches (610 mm). Framing Depth: 23 inches (584 mm). Glass Size: 36 inches x 24-1/2 inches (914 mm x 622 mm).
				2. BTU/Hour Input: 37,000 (10.8 kW).
		1. Slim Line Gas Fireplace: SL-3X, SL-5/5X, SL-7/7X, SL-9/9X

\*\* NOTE TO SPECIFIER \*\* Delete controls if not required.

* + - 1. Controls: Smart-Stat – Remote (SL-3, SL-5, SL-7, SL-9 models)
			2. Controls: WSK200 – Wall Switch (SL-3, SL-5, SL-7, SL-9 models)
			3. Controls: RCT-MLT - Remote (SL-3, SL-5, SL-7, SL-9 models)
			4. Controls: WSK-MLT - Wall Switch (SL-3, SL-5, SL-7, SL-9 models)
			5. RC300 – Remote (X collection models, included standard)
			6. RC200 – Remote (X collection models)
			7. RC100 - Wall Control (X collection models)

\*\* NOTE TO SPECIFIER \*\* Delete fronts-doors if not required.

* + - 1. Front- Full View Firescreen front in black
			2. Front- Arcadia- Black
			3. Front- Arcadia- Graphite
			4. Front- Arcadia- New Bronze
			5. Front- Halston - Black
			6. Front- Halston - Graphite
			7. Front- Halston - New Bronze
			8. Front- Chateau- Black
			9. Front- Chateau- Graphite
			10. Front- Chateau- New Bronze
			11. Front - Clean Face Kit- Black
			12. Front - Clean Face Kit- Graphite
			13. Front - Clean Face Kit- New Bronze

\*\* NOTE TO SPECIFIER \*\* An optional metal brick look refractory kit is available to change the look of the firebox. Delete refractory if not required.

* + - 1. Refractory: Ceramic Brick Style (SL-3, SL-5, SL-7, SL-9 models)
			2. Refractory: Reflective Ceramic- Black (SL-3, SL-5, SL-7, SL-9 models)
			3. Refractory: Reflective Ceramic- Black ( X collection models)

\*\* NOTE TO SPECIFIER \*\* Delete Trim Kits not required

* + - 1. Trim Kit - Three sided in black
			2. Trim Kit - Four sided in black
			3. Trim Kit - Three sided in stainless steel
			4. Trim Kit - Four sided in stainless steel

\*\* NOTE TO SPECIFIER \*\* Delete Heat Management not required

* + - 1. Zone Heat Distribution Kit
			2. Home Heat Distribution Kit

\*\* NOTE TO SPECIFIER \*\* Select mantel from available in mantels Article.

* + - 1. Wood Mantels: As specified.

\*\* NOTE TO SPECIFIER \*\* Select stone surrounds from available in stone surrounds Article.

* + - 1. Stone Surrounds: As specified.

\*\* NOTE TO SPECIFIER \*\* Select cast mantels from available in cast mantels Article.

* + - 1. Cast Mantels: As specified.

\*\* NOTE TO SPECIFIER \*\* Select mantel shelf from available in mantel shelf Article.

* + - 1. Mantel Shelf: As specified.

\*\* NOTE TO SPECIFIER \*\* Delete model not required.

* + - 1. Model SL-3X as manufactured by Heat & Glo.
				1. Size: Unit Front Width: 33 inches (838 mm). Framing Front Width: 34 inches (864 mm). Unit Back Width: 22-3/4 inches (578 mm). Framing Back Width: 34 inches (864 mm). Unit Height: 32-3/8 inches (822 mm). Framing Height: 34-3/4 inches (882 mm). Unit Depth: 16-1/4 inches (413 mm). Framing Depth: 16-1/4 inches (413 mm). Glass Size: 24-1/8 inches x 16 inches (613 mm x 406 mm).
				2. BTU/Hour Input: 11,500 - 21,000

\*\* NOTE TO SPECIFIER \*\* Contact manufacturer for test results.

* + - * 1. Efficiency: Steady State \_\_%, AFUE \_\_%, Canada EnerGuide \_\_%.
			1. Model SL-5 / SL-5X as manufactured by Heat & Glo.
				1. Size: Unit Front Width: 36 inches (913 mm). Framing Front Width: 37 inches (940 mm). Unit Back Width: 25-3/4 inches (653 mm). Framing Back Width: 37 inches (940 mm). Unit Height: 34-3/8 inches (873 mm). Framing Height: 34-3/4 inches (882 mm). Unit Depth: 16-5/6 inches (415 mm). Framing Depth: 16-1/4 inches (413 mm). Glass Size: 27-3/16 inches x 18-1/16 inches (691 mm x 459 mm).
				2. BTU/Hour Input: 14,900-21,000 (SL 5) 14,500-27,500 (SL-5X)

\*\* NOTE TO SPECIFIER \*\* Contact manufacturer for test results.

* + - * 1. Efficiency: Steady State \_\_%, AFUE \_\_%, Canada EnerGuide \_\_%.
			1. Model SL-7 / SL-7X as manufactured by Heat & Glo.
				1. Size: Unit Front Width: 41 inches (1041 mm). Framing Front Width: 42 inches (1067 mm). Unit Back Width: 30-3/4 inches (781 mm). Framing Back Width: 42 inches (1067 mm). Unit Height: 37-7/8 inches (962 mm). Framing Height: 38-1/4 inches (972 mm). Unit Depth: 16-5/16 inches (415 mm). Framing Depth: 16-1/4 inches (413 mm). Glass Size: 32-1/16 inches x 21-1/2 inches (814 mm x 546 mm).
				2. BTU/Hour Input: 17,500-25,000 (SL-7) 17,500-30,500 (SL-7X)

\*\* NOTE TO SPECIFIER \*\* Contact manufacturer for test results.

* + - * 1. Efficiency: Steady State \_\_%, AFUE \_\_%, Canada EnerGuide \_\_%.
			1. Model SL-9 / SL-9X as manufactured by Heat & Glo.
				1. Size: Unit Front Width: 48 inches (1218 mm). Framing Front Width: 49 inches (1245 mm). Unit Back Width: 37-3/4 inches (959 mm). Framing Back Width: 49 inches (1245 mm). Unit Height: 41-7/8 inches (1063 mm). Framing Height: 40-1/4 inches (972 mm). Unit Depth: 16-5/6 inches (415 mm). Framing Depth: 16-1/4 inches (415 mm). Glass Size: 39-1/16 inches x 23-9/16 inches (992 mm x 599 mm).
				2. BTU/Hour Input: 23,500-30,000 (SL-9) 18,000-35,000 (SL-9X)

\*\* NOTE TO SPECIFIER \*\* Contact manufacturer for test results.

* + - * 1. Efficiency: Steady State \_\_%, AFUE \_\_%, Canada EnerGuide \_\_%.
		1. ST-550T See-Through Gas Fireplace:

\*\* NOTE TO SPECIFIER \*\* Delete controls if not required.

* + - 1. Controls: WSK200.
			2. Controls: Smart-Stat.
			3. Controls: RCT-MLT.

\*\* NOTE TO SPECIFIER \*\* Delete fronts-doors if not required.

* + - 1. Front-Door: Black Aero Front.
			2. Front-Door: Graphite Aero Front.
			3. Front-Door: New Bronze Aero Front.
			4. Front-Door: Black Halston Front.
			5. Front-Door: Graphite Halston Front.
			6. Front-Door: New Bronze Halston Front.
			7. Front-Door: Black Chateau Deluxe Front.
			8. Front-Door: Graphite Chateau Deluxe Front.
			9. Front-Door: New Bronze Chateau Deluxe Front.
			10. Front-Door: Black Clean Face Front.
			11. Front-Door: Graphite Clean Face Front.
			12. Front-Door: New Bronze Clean Face Front.

\*\* NOTE TO SPECIFIER \*\* Select mantels from available in mantels Article.

* + - 1. Mantels: As specified.

\*\* NOTE TO SPECIFIER \*\* Select mantel shelves from available in mantel shelve Article. Bennington and Covington only.

* + - 1. Mantel Shelf: As specified.
			2. Model ST-550T as manufactured by Heat & Glo.
				1. Size: Unit Front Width: 37-5/8 inches (956 mm). Framing Front Width: 38-1/8 inches (968 mm). Unit Back Width: 37-5/8 inches (956 mm). Framing Back Width: 38-1/8 inches (968 mm). Unit Height: 34-1/2 inches (876 mm). Framing Height: 34-3/4 inches (883 mm). Unit Depth: 16 inches (406 mm). Framing Depth: 15 inches (381 mm). Glass Size: 31 inches x 21 inches (787 mm x 533 mm).
				2. BTU/Hour Input: 21,000 (6.2 kW).
		1. Crescent II Gas Fireplace:

\*\* NOTE TO SPECIFIER \*\* Delete control if not required.

* + - 1. Controls: 4041-128. On/off, flame high/low, auxiliary function (accent lighting).

\*\* NOTE TO SPECIFIER \*\* Delete fronts-doors not required.

* + - 1. Front - Door: Black Designer Classic Front.
			2. Front - Door: Bronze Essence Front.

\*\* NOTE TO SPECIFIER \*\* Delete panel not required.

* + - 1. Panel: Bronze Classic Decorative Panel
			2. Panel: Bronze Mission Decorative Panel
			3. Panel: Bronze Waverly Decorative Panel

\*\* NOTE TO SPECIFIER \*\* Delete cabinet if not required.

* + - 1. Cabinets: Bella Cabinet.

\*\* NOTE TO SPECIFIER \*\* Delete cabinet finish not required.

* + - * 1. Finish: Maple Auburn.
				2. Finish: Maple Chocolate.
				3. Finish: Maple Ginger.
				4. Finish: Maple Honey.
				5. Finish: Maple Natural.
				6. Finish: Oak Chocolate.
				7. Finish: Oak Ginger.
				8. Finish: Oak Honey.
				9. Finish: Oak Natural.
				10. Finish: Primed wood fiber.
			1. Model Crescent II as manufactured by Heat & Glo.
				1. Size: Unit Front Width: 23-1/4 inches (591 mm). Framing Front Width: 24-1/2 inches (622 mm). Unit Back Width: 24-1/2 inches (622 mm). Framing Back Width: 24-1/2 inches (622 mm). Unit Height: 30-3/4 inches (781 mm). Framing Height: 37 inches (940 mm). Unit Depth: 15-1/8 inches (384 mm). Framing Depth: 15-5/8 inches (397 mm). Glass Size: 15-1/2 inches x 21 inches (394 mm x 533).
				2. BTU/Hour Input: 11,500 (3.4 kW).

\*\* NOTE TO SPECIFIER \*\* New product offering, contact Manufacturer for more information. Delete if not required.

* + 1. Gateway Gas Fireplace: Contact manufacturer.

\*\* NOTE TO SPECIFIER \*\* Delete if not required.

* 1. MANUFACTURED OUTDOOR GAS FIREPLACES

\*\* NOTE TO SPECIFIER \*\* Bolster your favorite room and upgrade your outdoor living space. The Twilight Modern is an evolution of the industry's first indoor/outdoor see-through fireplace, and delivers impressive fireside views whether relaxing inside or socializing outside. No chimney or venting required. Delete if not required.

* + 1. Twilight Modern Gas Fireplace:

\*\* NOTE TO SPECIFIER \*\* Delete if not required.

* + - 1. Controls: WSK21

\*\* NOTE TO SPECIFIER \*\* An added level of function and convenience in a remote control fire fireplaces, stoves, inserts and gas logs with or without line power. Battery-powered or hardwired receiver. Includes: on/off, temperature readout, thermostat mode, timer mode. Delete if not required.

* + - 1. Controls: Smart-Stat.

\*\* NOTE TO SPECIFIER \*\* Delete front-door style and finish not required.

* + - 1. Fronts-Doors: Black Basic Front.
			2. Fronts-Doors: Black Contemporary front with built-in, overlapping surround.
			3. Fronts-Doors: Fog Contemporary front with built-in, overlapping surround.

\*\* NOTE TO SPECIFIER \*\* Delete media not required.

* + - 1. Media: Glass Media, Crystal.
			2. Media: Glass Media, Black.
			3. Media: Glass Media, Amber.
			4. Model TWILIGHT-II-MOD as manufactured by Heat & Glo.
				1. Unit Front Width: 43 inches (1092 mm).
				2. Framing Front Width: 44 inches (1118 mm).
				3. Unit Back Width: 43 inches (1092 mm).
				4. Framing Back Width: 44 inches (1118 mm).
				5. Unit Height - In: 40-3/4 inches (1035 mm).
				6. Unit Height - Out: 46-7/8 inches (1191 mm).
				7. Framing Height - In: 41-1/4 inches (1048 mm).
				8. Framing Height - Out: 47-5/8 inches (1210 mm).
				9. Unit Depth: 24 inches (610 mm).
				10. Framing Depth: 23 inches (584 mm).
				11. Glass Size: 35-5/8 inches (905 mm) x 21-1/2 inches (546 mm).
				12. BTU/Hour Input: 38,000 NG (11.1 kW).

\*\* NOTE TO SPECIFIER \*\* Add warmth and beauty to two spaceswith one fireplace. The Twilight II is the world's first see-thru indoor/outdoor gas fireplace. Enjoy the fire all year long, and from either side. An advanced design exceeds both window and gas fireplace standards, and rugged construction ensures impressive, consistent performance. Delete if not required.

* + 1. Twilight II Gas Fireplace:

\*\* NOTE TO SPECIFIER \*\* Designed exclusively for fireplaces with IntelliFire™, our state-of-the-art intermittent pilot ignition system. Includes: on/off, auto battery backup, battery strength indicator, fan speed, flame control, pilot activation. Delete if not required.

* + - 1. Controls: WSK200.

\*\* NOTE TO SPECIFIER \*\* An added level of function and convenience in a remote control fire fireplaces, stoves, inserts and gas logs with or without line power. Battery-powered or hardwired receiver. Includes: on/off, temperature readout, thermostat mode, timer mode. Delete if not required.

* + - 1. Controls: Smart-Stat.

\*\* NOTE TO SPECIFIER \*\* Delete front-door style and finish not required.

* + - 1. Fronts-Doors: Black Basic Front.
			2. Fronts-Doors: Black Contemporary front with built-in, overlapping surround.
			3. Fronts-Doors: Fog Contemporary front with built-in, overlapping surround.
			4. Model TWILIGHTII as manufactured by Heat & Glo.
				1. Unit Front Width: 43 inches (1092 mm).
				2. Framing Front Width: 44 inches (1118 mm).
				3. Unit Back Width: 43 inches (1092 mm).
				4. Framing Back Width: 44 inches (1118 mm).
				5. Unit Height - In: 40-3/4 inches (1035 mm).
				6. Unit Height - Out: 46-7/8 inches (1191 mm).
				7. Framing Height - In: 41-1/4 inches (1048 mm).
				8. Framing Height - Out: 47-5/8 inches (1210 mm).
				9. Unit Depth: 24 inches (610 mm).
				10. Framing Depth: 23 inches (584 mm).
				11. Glass Size: 35-5/8 inches (905 mm) x 21-1/2 inches (546 mm).
				12. BTU/Hour Input: 38,000 NG (11.1 kW).

\*\* NOTE TO SPECIFIER \*\* The Dakota artfully blends style, function and utility with outdoor living. A rugged design loaded with advanced technology make the Dakota an enticing outdoor fireplace for years to come. Delete if not required.

* + 1. Dakota Gas Fireplace:

\*\* NOTE TO SPECIFIER \*\* Delete Refractory design not required.

* + - 1. Refractory: Traditional Refractory.
			2. Refractory: Herringbone Refractory.
			3. Model Dakota as manufactured by Heat & Glo.
				1. Unit Front Width: 48 inches (1219 mm).
				2. Framing Front Width: 49 inches (1245 mm).
				3. Unit Back Width: 31 inches (787 mm).
				4. Framing Back Width: 49 inches (1245 mm).
				5. Unit Height: 40 inches (1016 mm).
				6. Framing Height: 43-7/8 inches (1114 mm).
				7. Unit Depth: 23-1/4 inches (591 mm).
				8. Framing Depth: 24-1/8 inches (613 mm).
				9. Glass Size: 26-13/16 inches (681 mm) x 42-1/2 inches (1080 mm).
				10. BTU/Hour Input: 60,000 (17.6 kW).

\*\* NOTE TO SPECIFIER \*\* The Carolina's compact footprint offers versatile installation opportunities. And, this attractive unit is packed with advanced technology, like the IntelliFire™ Plus auto-ignition system and Fire Brick technology for up to 25% more radiant heat. Extend your summer season with style. Bring the Carolina home. Delete if not required.

* + 1. Carolina:

\*\* NOTE TO SPECIFIER \*\* Designed exclusively for fireplaces with IntelliFire™, our state-of-the-art intermittent pilot ignition system. Features a simple, single mode function and is specifically designed for wall placement ensuring a great fire is just a tap of the switch away. Delete if not required.

* + - 1. Controls: IntelliFire Plus RC100.

\*\* NOTE TO SPECIFIER \*\* Combines an easy-to-use and intuitive control panel with a stylish and ergonomic design. Since it utilizes wireless control, it has the flexibility for wall placement anywhere in the room, or use as a remote only. Auto Battery Backup, Pilot Activation, On/Off, 5 Step Flame Height, Fan Speed, Child Lock, Wall Docking Station. Delete if not required.

* + - 1. Controls: IntelliFire Plus RC200.

\*\* NOTE TO SPECIFIER \*\* Delete front-door style if not required.

* + - 1. Fronts-Doors: DSCAR3642 Front.

\*\* NOTE TO SPECIFIER \*\* Delete model not required.

* + - 1. Model CAROLINA-36 as manufactured by Heat & Glo.
				1. Unit Front Width: 44 inches (1118 mm).
				2. Framing Front Width: 48 inches (1219 mm).
				3. Unit Back Width: 44 inches (1118 mm).
				4. Framing Back Width: 48 inches (1219 mm).
				5. Unit Height: 42-1/2 inches (1080 mm).
				6. Framing Height: 42-1/2 inches (1080 mm).
				7. Unit Depth: 17 inches (432 mm).
				8. Framing Depth: 17 inches (432 mm).
				9. Glass Size: 33-3/8 inches (848 mm) x 28-7/8 inches (733 mm).
				10. BTU/Hour Input: 55,000 (16.1 kW).
			2. Model CAROLINA-42 as manufactured by Heat & Glo.
				1. Unit Front Width: 50 inches (1270 mm).
				2. Framing Front Width: 54 inches (1372 mm).
				3. Unit Back Width: 50 inches (1270 mm).
				4. Framing Back Width: 54 inches (1372 mm).
				5. Unit Height: 50-1/2 inches (1283 mm).
				6. Framing Height: 50-1/2 inches (1283 mm).
				7. Unit Depth: 17 inches (432 mm).
				8. Framing Depth: 17 inches (432 mm).
				9. Glass Size: 39-1/8 inches (994 mm) x 33-3/4 inches (857 mm).
				10. BTU/Hour Input: 65,000 (19 kW).

\*\* NOTE TO SPECIFIER \*\* The Villa Gas is a versatile outdoor gas fireplace at a value price. This compact unit can easily be installed on decks or patios. A stainless steel surround withstands the elements, and complements an outdoor kitchen or contemporary living space. Delete if not required.

* + 1. Outdoor Lifestyles Villa Gas Fireplace:

\*\* NOTE TO SPECIFIER \*\* Delete Fronts-doors if not required.

* + - 1. Front-Door: Stainless Steel Operable Doors.

\*\* NOTE TO SPECIFIER \*\* Delete Refractory design not required.

* + - 1. Refractory: Traditional Refractory.
			2. Refractory: Herringbone Refractory.

\*\* NOTE TO SPECIFIER \*\* Delete model not required.

* + - 1. Model VILLA Gas-36 as manufactured by Heat & Glo.
				1. Unit Front Width: 41 inches (1041 mm).
				2. Framing Front Width: 42 inches (1067 mm).
				3. Unit Back Width: 23-3/4 inches (603 mm).
				4. Framing Back Width: 42 inches (1067 mm).
				5. Unit Height: 39-1/2 inches (1003 mm).
				6. Framing Height: 39-3/4 inches (1010 mm).
				7. Unit Depth: 21-3/8 inches (543 mm).
				8. Framing Depth: 21-1/2 inches (546 mm).
				9. Viewing Area: 36 inches (914 mm) x 20-7/8 inches (530 mm).
				10. BTU/Hour Input: 40,000 (11.7 kW).
			2. Model VILLA Gas-42 as manufactured by Heat & Glo.
				1. Unit Front Width: 47 inches (1194 mm).
				2. Framing Front Width: 48 inches (1219 mm).
				3. Unit Back Width: 29-3/4 inches (756 mm).
				4. Framing Back Width: 48 inches (1219 mm).
				5. Unit Height: 39-1/2 inches (1003 mm).
				6. Framing Height: 39-3/4 inches (1010 mm).
				7. Unit Depth: 21-3/8 inches (543 mm).
				8. Framing Depth: 21-1/2 inches (546 mm).
				9. Glass Size: 42 inches (1067 mm) x 20-7/8 inches (530 mm).
				10. BTU/Hour Input: 42,000 (12.3 kW).

\*\* NOTE TO SPECIFIER \*\* The Palazzo See-through is a new kind of outdoor fireplacea linear design with a clean look that provides a contemporary focal point in an outdoor setting. This eye-catching fireplace is tough, built with marine-grade stainless steel that is rust-resistant even in the harshest conditions. A tempered glass wind guard keeps the flames full and lively, while an industry-first Power Screen provides safety.
The contemporary Palazzo outdoor linear model in a single sided configuration. Perfect for residential and commercial projects calling for a unique focal point for an outdoor living space or meeting area.
Delete if not required.

* + 1. Outdoor Lifestyles Palazzo Series Modern Fireplace:
			1. Power Screen (Comes Standard).
			2. LED Lighting.

\*\* NOTE TO SPECIFIER \*\* Delete media options not required.

* + - 1. Media: Glass Media, Crystal.
			2. Media: Glass Media, Cobalt.
			3. Media: Glass Media, Ebony.
			4. Media: Glass Media, Scarlet.
			5. Media: Glass Media, Amber.

\*\* NOTE TO SPECIFIER \*\* Delete models not required.

* + - 1. Model Palazzo Single Sided as manufactured by Heat & Glo.
				1. Unit Front Width: 59-7/8 inches (1521 mm).
				2. Framing Front Width: 60 inches (1524 mm).
				3. Unit Back Width: 59-7/8 inches (1521 mm).
				4. Framing Back Width: 60 inches (1524 mm).
				5. Unit Height: 45-1/2 inches (1156 mm).
				6. Framing Height: 62-3/8 inches (1584 mm).
				7. Unit Depth: 18-5/8 inches (473 mm).
				8. Framing Depth: 18-1/8 inches (460 mm).
				9. Glass Size: 48 inches (1219 mm) x 13-7/8 inches (352 mm).
				10. BTU/Hour Input: 43,000 (12.6 kW).
			2. Model Palazzo See-Through as manufactured by Heat & Glo.
				1. Unit Front Width: 59-7/8 inches (1521 mm).
				2. Framing Front Width: 60 inches (1524 mm).
				3. Unit Back Width: 59-7/8 inches (1521 mm).
				4. Framing Back Width: 60 inches (1524 mm).
				5. Unit Height: 45-1/2 inches (1156 mm).
				6. Framing Height: 62-3/8 inches (1584 mm).
				7. Unit Depth: 18-1/4 inches (464 mm).
				8. Framing Depth: 17 inches (432 mm).
				9. Glass Size: 48 inches (1219 mm) x 13-7/8 inches (352 mm).
				10. BTU/Hour Input: 43,000 (12.6 kW).

\*\* NOTE TO SPECIFIER \*\* Delete if not required.

* 1. GAS FIREPLACE MANTELS AND FIREPLACE SURROUNDS

\*\* NOTE TO SPECIFIER \*\* Dress up your fireplace with mantels and surrounds that complement any style. Heat & Glo's collection of wood mantels display simple elegance and classic beauty.

* + 1. Wood Mantels and Surrounds as manufactured by Heat & Glo.

\*\* NOTE TO SPECIFIER \*\* Delete style and finish not required.

* + - 1. Belair.
				1. Finish: Maple Auburn.
				2. Finish: Maple Chocolate.
				3. Finish: Maple Ginger.
				4. Finish: Maple Honey.
				5. Finish: Maple Natural.
				6. Finish: Oak Chocolate.
				7. Finish: Oak Ginger.
				8. Finish: Oak Honey.
				9. Finish: Oak Natural.
				10. Finish: Primed wood fiber.
			2. Bella Cabinet.
				1. Finish: Maple Auburn.
				2. Finish: Maple Chocolate.
				3. Finish: Maple Ginger.
				4. Finish: Maple Honey.
				5. Finish: Maple Natural.
				6. Finish: Oak Chocolate.
				7. Finish: Oak Ginger.
				8. Finish: Oak Honey.
				9. Finish: Oak Natural.
				10. Finish: Primed wood fiber.
			3. Bridgeport.
				1. Finish: Oak Chocolate.
				2. Finish: Oak Ginger.
				3. Finish: Oak Honey.
				4. Finish: Oak Natural.
				5. Finish: Primed wood fiber.
			4. Fairfield.
				1. Finish: Maple Auburn.
				2. Finish: Maple Chocolate.
				3. Finish: Maple Ginger.
				4. Finish: Maple Honey.
				5. Finish: Maple Natural.
				6. Finish: Oak Chocolate.
				7. Finish: Oak Ginger.
				8. Finish: Oak Honey.
				9. Finish: Oak Natural.
				10. Finish: Primed wood fiber.
			5. Hastings.
				1. Finish: Oak Chocolate.
				2. Finish: Oak Ginger.
				3. Finish: Oak Honey.
				4. Finish: Oak Natural.
				5. Finish: Primed wood fiber.
			6. Kenwood Corner.
				1. Finish: Maple Auburn.
				2. Finish: Maple Chocolate.
				3. Finish: Maple Ginger.
				4. Finish: Maple Honey.
				5. Finish: Maple Natural.
				6. Finish: Oak Chocolate.
				7. Finish: Oak Ginger.
				8. Finish: Oak Honey.
				9. Finish: Oak Natural.
				10. Finish: Primed wood fiber.
			7. Kenwood Corner with Base.
				1. Finish: Maple Auburn.
				2. Finish: Maple Chocolate.
				3. Finish: Maple Ginger.
				4. Finish: Maple Honey.
				5. Finish: Maple Natural.
				6. Finish: Oak Chocolate.
				7. Finish: Oak Ginger.
				8. Finish: Oak Honey.
				9. Finish: Oak Natural.
				10. Finish: Primed wood fiber.
			8. Kenwood Wall Cabinet.
				1. Finish: Maple Auburn.
				2. Finish: Maple Chocolate.
				3. Finish: Maple Ginger.
				4. Finish: Maple Honey.
				5. Finish: Maple Natural.
				6. Finish: Oak Chocolate.
				7. Finish: Oak Ginger.
				8. Finish: Oak Honey.
				9. Finish: Oak Natural.
				10. Finish: Primed wood fiber.
			9. Kenwood Wall Cabinet with Base.
				1. Finish: Maple Auburn.
				2. Finish: Maple Chocolate.
				3. Finish: Maple Ginger.
				4. Finish: Maple Honey.
				5. Finish: Maple Natural.
				6. Finish: Oak Chocolate.
				7. Finish: Oak Ginger.
				8. Finish: Oak Honey.
				9. Finish: Oak Natural.
				10. Finish: Primed wood fiber.
			10. Mount Vernon.
				1. Finish: Maple Auburn.
				2. Finish: Maple Chocolate.
				3. Finish: Maple Ginger.
				4. Finish: Maple Honey.
				5. Finish: Maple Natural.
				6. Finish: Oak Chocolate.
				7. Finish: Oak Ginger.
				8. Finish: Oak Honey.
				9. Finish: Oak Natural.
				10. Finish: Primed wood fiber.
			11. Newport.
				1. Finish: Oak Chocolate.
				2. Finish: Oak Ginger.
				3. Finish: Oak Honey.
				4. Finish: Oak Natural.
				5. Finish: Primed wood fiber.
			12. Philips Hall.
				1. Finish: Alder Auburn.
				2. Finish: Alder Chocolate.
				3. Finish: Alder Ginger.
				4. Finish: Alder Honey.
				5. Finish: Alder Natural.
				6. Finish: Maple Auburn.
				7. Finish: Maple Chocolate.
				8. Finish: Maple Ginger.
				9. Finish: Maple Honey.
				10. Finish: Maple Natural.
				11. Finish: Oak Chocolate.
				12. Finish: Oak Ginger.
				13. Finish: Oak Honey.
				14. Finish: Oak Natural.
				15. Finish: Primed wood fiber.
			13. Plymouth.
				1. Finish: Maple Auburn.
				2. Finish: Maple Chocolate.
				3. Finish: Maple Ginger.
				4. Finish: Maple Honey.
				5. Finish: Maple Natural.
				6. Finish: Oak Chocolate.
				7. Finish: Oak Ginger.
				8. Finish: Oak Honey.
				9. Finish: Oak Natural.
				10. Finish: Primed wood fiber.
			14. Portico with Filler.
				1. Finish: Alder Auburn.
				2. Finish: Alder Chocolate.
				3. Finish: Alder Ginger.
				4. Finish: Alder Honey.
				5. Finish: Alder Natural.
				6. Finish: Maple Auburn.
				7. Finish: Maple Chocolate.
				8. Finish: Maple Ginger.
				9. Finish: Maple Honey.
				10. Finish: Maple Natural.
				11. Finish: Oak Chocolate.
				12. Finish: Oak Ginger.
				13. Finish: Oak Honey.
				14. Finish: Oak Natural.
				15. Finish: Primed wood fiber.
			15. Portico without Filler.
				1. Finish: Alder Auburn.
				2. Finish: Alder Chocolate.
				3. Finish: Alder Ginger.
				4. Finish: Alder Honey.
				5. Finish: Alder Natural.
				6. Finish: Maple Auburn.
				7. Finish: Maple Chocolate.
				8. Finish: Maple Ginger.
				9. Finish: Maple Honey.
				10. Finish: Maple Natural.
				11. Finish: Oak Chocolate.
				12. Finish: Oak Ginger.
				13. Finish: Oak Honey.
				14. Finish: Oak Natural.
				15. Finish: Primed wood fiber.
			16. Portico with Filler Painted.
				1. Finish: Alder Auburn.
				2. Finish: Alder Chocolate.
				3. Finish: Alder Ginger.
				4. Finish: Alder Honey.
				5. Finish: Alder Natural.
				6. Finish: Maple Auburn.
				7. Finish: Maple Chocolate.
				8. Finish: Maple Ginger.
				9. Finish: Maple Honey.
				10. Finish: Maple Natural.
				11. Finish: Oak Chocolate.
				12. Finish: Oak Ginger.
				13. Finish: Oak Honey.
				14. Finish: Oak Natural.
				15. Finish: Primed wood fiber.
			17. Roseville.
				1. Finish: Maple Auburn.
				2. Finish: Maple Chocolate.
				3. Finish: Maple Ginger.
				4. Finish: Maple Honey.
				5. Finish: Maple Natural.
				6. Finish: Oak Chocolate.
				7. Finish: Oak Ginger.
				8. Finish: Oak Honey.
				9. Finish: Oak Natural.
				10. Finish: Primed wood fiber.
			18. Sonoma.
				1. Finish: Alder Auburn.
				2. Finish: Alder Chocolate.
				3. Finish: Alder Ginger.
				4. Finish: Alder Honey.
				5. Finish: Alder Natural.
				6. Finish: Maple Auburn.
				7. Finish: Maple Chocolate.
				8. Finish: Maple Ginger.
				9. Finish: Maple Honey.
				10. Finish: Maple Natural.
				11. Finish: Oak Chocolate.
				12. Finish: Oak Ginger.
				13. Finish: Oak Honey.
				14. Finish: Oak Natural.
				15. Finish: Primed wood fiber.
			19. Winchester.
				1. Finish: Oak Chocolate.
				2. Finish: Oak Ginger.
				3. Finish: Oak Honey.
				4. Finish: Oak Natural.
				5. Finish: Primed wood fiber.
			20. Yorktown.
				1. Finish: Oak Chocolate.
				2. Finish: Oak Ginger.
				3. Finish: Oak Honey.
				4. Finish: Oak Natural.
				5. Finish: Primed wood fiber.
			21. Parsons.
				1. Finish: Alder Auburn.
				2. Finish: Alder Chocolate.
				3. Finish: Alder Ginger.
				4. Finish: Alder Honey.
				5. Finish: Alder Natural.
				6. Finish: Maple Auburn.
				7. Finish: Maple Chocolate.
				8. Finish: Maple Ginger.
				9. Finish: Maple Honey.
				10. Finish: Maple Natural.
				11. Finish: Oak Chocolate.
				12. Finish: Oak Ginger.
				13. Finish: Oak Honey.
				14. Finish: Oak Natural.
				15. Finish: Primed wood fiber.

\*\* NOTE TO SPECIFIER \*\* Heat & Glo stone surround sets are the perfect design element to complement your fireplace. Available in granite, marble and slate, these fireplace surround sets feature elegance and quality. Delete if not required.

* + 1. Stone Surround Sets
			1. Absolute Black Granite.
			2. Beige Marble.
			3. Caledonia Granite.
			4. Green Granite.
			5. Marron Brown Marble.
			6. New Venetian Granite.
			7. Slate.
			8. Tan Brown Granite.
			9. Wheatfield Granite.

\*\* NOTE TO SPECIFIER \*\* Stylize your living space with a cast stone fireplace mantel and cast surround from Heat & Glo.

* + 1. Cast Mantels and Surrounds:
			1. Atlas.
			2. Avalon.
				1. Finish: Beige.
				2. Finish: Macchiato.
			3. Avalon with Overmantel.
				1. Finish: Beige.
				2. Finish: Macchiato.
			4. Biltmore.
				1. Finish: Beige.
				2. Finish: Macchiato.
			5. Biltmore with Overmantel.
				1. Finish: Beige.
				2. Finish: Macchiato.
			6. Hearst.
				1. Finish: Beige.
				2. Finish: Macchiato.
			7. Hearst with Overmantel.
				1. Finish: Beige.
				2. Finish: Macchiato.

\*\* NOTE TO SPECIFIER \*\* Accent the look of your Heat & Glo fireplace with a cast or wood mantel shelf. Whether it's for usability or for decor, a mantel shelf dresses up your fireplace perfectly.

* + 1. Mantel Shelves:

\*\* NOTE TO SPECIFIER \*\* Delete length not required.

* + - 1. Length: 48 inches (1219 mm)."
			2. Length: 59 inches (1499 mm).
			3. Length: 72 inches (1829 mm).

\*\* NOTE TO SPECIFIER \*\* Delete style and finish not required.

* + - 1. Everest.

\*\* NOTE TO SPECIFIER \*\* Refer to manufacturer's literature. Delete if not required.

* + - * 1. Finish:
			1. Bennington.
				1. Finish: Maple Auburn.
				2. Finish: Maple Chocolate.
				3. Finish: Maple Ginger.
				4. Finish: Maple Honey.
				5. Finish: Maple Natural.
				6. Finish: Oak Chocolate.
				7. Finish: Oak Ginger.
				8. Finish: Oak Honey.
				9. Finish: Oak Natural.
				10. Finish: Primed wood fiber.
			2. Covington.
				1. Finish: Oak Chocolate.
				2. Finish: Oak Ginger.
				3. Finish: Oak Honey.
				4. Finish: Oak Natural.
				5. Finish: Primed wood fiber.
			3. St Cloud.
				1. Finish: Oak Chocolate.
				2. Finish: Oak Ginger.
				3. Finish: Oak Honey.
				4. Finish: Oak Natural.
				5. Finish: Alder Auburn.
				6. Finish: Alder Chocolate.
				7. Finish: Alder Ginger.
				8. Finish: Alder Honey.
				9. Finish: Alder Natural.
				10. Finish: Maple Auburn.
				11. Finish: Maple Chocolate.
				12. Finish: Maple Ginger.
				13. Finish: Maple Honey.
				14. Finish: Maple Natural.
				15. Finish: Primed wood fiber.

\*\* NOTE TO SPECIFIER \*\* Delete if not required.

\*\* NOTE TO SPECIFIER \*\* Take convenience to a new level with fireplace remote controls. Simply point and click to start enjoying the comfort of a fire in your home. Take a look at our catalog to find a remote product that will work best for you. Delete if not required.

* + 1. Controls:
			1. Wall Switches.
			2. Wall Mounted Controls.

\*\* NOTE TO SPECIFIER \*\* Offering both decorative and traditional gas termination caps, Heat & Glo can help you polish your fireplace system with the perfect finishing touch. Delete if not required.

* + 1. Termination Caps: Gas.

\*\* NOTE TO SPECIFIER \*\* Delete termination cap not required.

* + - 1. Horizontal Termination.
			2. Firebrick Termination.
			3. HP Termination.
			4. High-Rise Termination.
			5. Basement Termination.
			6. High Wind Termination.
			7. Decorative Radius Termination.
			8. Safety Shield Termination.
			9. Octagon Shroud Termination.
			10. Square Shroud Termination.
			11. Terracotta Termination.
			12. Decorative Shroud Termination.
			13. Round Termination.
			14. Square Termination.
			15. Decorative Square Termination.

\*\* NOTE TO SPECIFIER \*\* Circulating fans not available for all models. Refer to manufacturer's literature for model fan ready for add-on of electric fan.

* + 1. Circulating Fans: Manufacturer's standard circulating fan compatible with specified fireplace.
1. EXECUTION
	1. EXAMINATION
		1. Do not begin installation until substrates have been properly prepared.
		2. If substrate preparation is the responsibility of another installer, notify Architect of unsatisfactory preparation before proceeding.
	2. PREPARATION
		1. Clean surfaces thoroughly prior to installation.
		2. Prepare surfaces using the methods recommended by the manufacturer for achieving the best result for the substrate under the project conditions.
	3. INSTALLATION
		1. Install in accordance with manufacturer's instructions, ANSI Z21.44 and the requirements of authorities having jurisdiction.
		2. Use manufacturer's guidelines for minimum clearances to combustibles, walls, and finishes.
		3. Anchor all components firmly in position for long life under hard use.
	4. FIELD QUALITY CONTROL
		1. Upon completion of installation, visually inspect all exposed surfaces. Touch up scratches and abrasions with touch-up paint recommended by the manufacturer, make imperfections invisible to the unaided eye from a distance of 5 feet (1.5m).
		2. Test for proper operation, control and safety devices.
		3. Complete Installer's Warranty Validation Card.
	5. PROTECTION
		1. Protect installed products until completion of project.

END OF SECTION